{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["MCD","SCD","Abbreviations"],"not_rendered":{"images":15,"external_links":2,"defined_names":5,"comments":20},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"MCD","index":0,"n_rows":22,"n_cols":25,"rows_kept":22,"merged":[[0,0,0,24],[1,0,1,24],[2,13,2,18],[3,8,3,9],[5,15,5,24],[6,16,6,24],[7,0,7,24],[7,42,7,62],[7,63,7,83],[7,84,7,104],[7,105,7,125],[7,126,7,146],[7,147,7,167],[7,168,7,188],[7,189,7,209],[7,210,7,230],[7,231,7,251],[7,252,7,255],[11,5,11,14],[11,24,12,24],[13,21,13,23],[14,21,14,23],[15,21,15,23],[16,21,16,23],[17,21,17,23],[18,21,18,23]],"flags":["formulas_cached_only"]}
["Material Composition Declaration "]
["Supplier or Manufacturing Site Information"]
["Contact Name",null,"Yun Ding","Contact Title",null,"QS Engineer",null,"Contact Phone",null,"86-21-50802030",null,"Contact Email/Fax",null,"yun_ding@giantec-semi.com"]
["Company Name",null,"Giantec ","Name of person certifying",null,"Frank zhou","Certifying Title",null,"QRA Director",null,"Certifying Phone",null,"86-21-50802030",null,"Certifying Email",null,"Frank_Zhou@giantec-semi.com"]
["Part Category",null,"IC","Part Name","EEPROM",null,"Package Family",null,"MSOP",null,"Pin count",null,8,null,"Part weight (mg)",null,{"v":28.50524051663516,"d":"28.505"}]
["Part Number(s)",null,"GT24C**-2SLI-TR"]
["Alternative Recommended Item",null,null,"NA",null,"Alternative Item Name",null,"NA",null,"Availability Date ",null,"NA","Alternative Part Comments",null,null,"NA"]
["Manufacturing Process Information"]
["Terminal Plating/Grid Array Material Composition",null,null,2,"Terminal Plating Thickness (um)",null,null,"7.5~17","Terminal Base Alloy",null,"C7025","J-STD-020 Moisture",null,1,"Maximum Reflow Temp. ",null,"260 C"]
["Maximum temp. duration (sec)",null,null,10,"Maximum cycles for Reflow",null,null,3,"Comment"]
[]
[null,null,"                  Homogeneous Material ",null,null,"3rd Party Analytical Testing result (ppm)",{"$nulls":10},"Compliance (Yes/No)",null,null,"                 3rd Party Analytical Testing",{"$nulls":4},"MSDS"]
["Item","Name","Vender","Type","Weight (mg)","Cd ","Pb","Hg","Cr-VI","PBBs","PBDEs","DEHP","BBP","DBP","DIBP","RoHS","JIG Level A","Exempt","Lab. Name","Report No.","Date","1.RoHS","2.Halogen","3.PFOS/PFOA"]
[1,"Leadframe","Mitsui","C7025+Ag",{"v":15.7541274,"d":"15.754"},"N.D.","N.D.","N.D.","Negative","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","Yes","Yes","No","SGS","TSNEC2201475001","2022-06-13"]
[2,"Die attach paste","SHOWA DENKO","EN4900G",{"v":0.045883068,"d":"0.046"},"N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","Yes","Yes","No","SGS","ETR22701026M17","2022-07-12"]
[3,"Copper Wire","NIPPON","EX-SERIES",{"v":0.0279351129455591,"d":"0.028"},"N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","Yes","Yes","No","SGS","ETR23101251","2023-01-16"]
[4,"Molding compound","SD","CEL-9240HF",{"v":12.1956853324896,"d":"12.196"},"N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","Yes","Yes","No","SGS","SHAEC22003258323\nSHAEC22003258324","2022-11-23"]
[5,"Lead finish \n(Matte Sn) on leadframe","Tinking","Sn 99.99%",{"v":0.2548932672,"d":"0.255"},"N.D.",53,"N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","Yes","Yes","No","SGS","SHAEC22002018506","2022-10-12"]
[6,"DIE","SMIC","silicon",{"v":0.226716336,"d":"0.227"},"N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","N.D.","Yes","Yes","No","CTI","A2220522292101005","2023-01-05"]
[]
[null,"Giantec fill in"]
[null,"Supplier or Manufacturing Site fill in",{"$nulls":11},"Final Compliance Judgement of GP",{"$nulls":3},"Yes",null,null,"No"]

{"sheet":"SCD","index":1,"n_rows":47,"n_cols":17,"rows_kept":47,"merged":[[0,0,0,18],[1,0,1,18],[5,6,5,18],[6,16,6,18],[7,0,7,18],[11,12,12,12],[11,13,12,13],[11,19,12,19],[13,0,40,0],[13,1,20,1],[13,2,20,2],[13,3,20,3],[13,4,20,4],[21,1,28,1],[21,2,28,2],[21,3,28,3],[21,4,28,4],[29,1,30,1],[29,2,30,2],[29,3,30,3],[29,4,30,4],[31,1,37,1],[31,2,37,2],[31,3,37,3],[31,4,37,4],[39,1,40,1],[39,2,40,2],[39,3,40,3],[39,4,40,4]],"flags":["formulas_cached_only"]}
["Substance Composition Declaration "]
["Supplier or Manufacturing Site Information"]
["Response Date",null,"NA","Contact Name",null,"Yun Ding","Contact Title",null,"QS Engineer",null,"Contact Phone",null,"86-21-50802030",null,"Contact Email/Fax",null,"yun_ding@giantec-semi.com"]
["Company Name",null,"Giantec ","Name of person certifying",null,"Frank zhou","Certifying Title",null,"QRA Director",null,"Certifying Phone",null,"86-21-50802030",null,"Certifying Email",null,"Frank_Zhou@giantec-semi.com"]
["Part Category",null,"IC","Part Name","EEPROM",null,"Package Family",null,"MSOP",null,"Pin count",null,8,null,"Part wight (mg)",null,{"v":28.50524051663516,"d":"28.5052405"}]
["Part Number(s)",null,"GT24C64A-2SLI-TR"]
["Alternative Recommended Item",null,null,"NA",null,"Alternative Item Name",null,"NA",null,"Availability Date ",null,"NA","Alternative Part Comments",null,null,"NA"]
["Manufacturing Process Information"]
["Terminal Plating/Grid Array Material Composition",null,null,2,"Terminal Plating Thickness (um)",null,null,"7.5~17","Terminal Base Alloy",null,"C7025","J-STD-020 Moisture",null,1,"Maximum Reflow Temp. ",null,"260 C"]
["Maximum temp. duration (sec)",null,null,10,"Maximum cycles for Reflow",null,null,3,"Comment",null,0]
[]
[null,null,"                  Homogeneous Material ",null,null,"JIG",null,null,"                   Substance",{"$nulls":3},"J/E%","%"]
["Item","Name","Vender","Type","Weight (mg)","Level","Category","Name","CAS","Weight (mg)","PPM","Exempt"]
["MSOP","Leadframe","Mitsui","C7025+Ag",{"v":15.7541274,"d":"15.754"},"Other",null,"Silicon(Si)","7440-21-3 ",{"v":0.08034604974000001,"d":"0.080"},{"v":2818.6413544944994,"d":"2,819"},"No",{"v":0.0051,"d":"0.51%"},{"v":0.0028186413544944995,"d":"0.282%"}]
[{"$nulls":5},"Other",null,"Nickel(Ni)","7440-02-0 ",{"v":0.38282529581999997,"d":"0.383"},{"v":13429.9970420032,"d":"13,430"},"No",{"v":0.0243,"d":"2.43%"},{"v":0.0134299970420032,"d":"1.343%"}]
[{"$nulls":5},"Other",null,"Magnesium(Mg)","7439-95-4",{"v":0.0157541274,"d":"0.016"},{"v":552.6747753910784,"d":"553"},"No",{"v":0.001,"d":"0.10%"},{"v":0.0005526747753910783,"d":"0.055%"}]
[{"$nulls":5},"Other",null,"Iron(Fe)","7439-89-6",{"v":0.00315082548,"d":"0.003"},{"v":110.53495507821566,"d":"111"},"No",{"v":0.0002,"d":"0.02%"},{"v":0.00011053495507821566,"d":"0.011%"}]
[{"$nulls":5},"Other",null,"Lead Plumbum(Pb)","7439-92-1",{"v":0.00078770637,"d":"0.001"},{"v":27.633738769553915,"d":"28"},"No",{"v":5e-05,"d":"0.01%"},{"v":2.7633738769553915e-05,"d":"0.003%"}]
[{"$nulls":5},"Other",null,"manganese(Mn)","7439-96-5 ",{"v":0.00078770637,"d":"0.001"},{"v":27.633738769553915,"d":"28"},"No",{"v":5e-05,"d":"0.01%"},{"v":2.7633738769553915e-05,"d":"0.003%"}]
[{"$nulls":5},"Other",null,"Copper(Cu)","7440-50-8",{"v":15.04834249248,"d":"15.048"},{"v":527914.945453558,"d":"527,915"},"No",{"v":0.9552,"d":"95.52%"},{"v":0.527914945453558,"d":"52.791%"}]
[{"$nulls":5},"Other",null,"Silver（Ag）","7440-22-4",{"v":0.22213319634,"d":"0.222"},{"v":7792.714333014204,"d":"7,793"},"No",{"v":0.0141,"d":"1.41%"},{"v":0.007792714333014204,"d":"0.779%"}]
[null,"Die attach paste","SHOWA DENKO","EN4900G",{"v":0.045883068,"d":"0.046"},"Other",null,"Silver"," 7440-22-4",{"v":0.03395347032,"d":"0.034"},{"v":1191.1308133037974,"d":"1,191 "},"No",{"v":0.74,"d":"74.00%"},{"v":0.0011911308133037975,"d":"0.119%"}]
[{"$nulls":5},"Other",null,"Acrylic resin","Trade secret",{"v":0.0041294761199999995,"d":"0.004"},{"v":144.86726107748888,"d":"145 "},"No",{"v":0.09,"d":"9.00%"},{"v":0.00014486726107748889,"d":"0.014%"}]
[{"$nulls":5},"Other",null,"Polybutadiene derivative ","Trade secret",{"v":0.0022941534,"d":"0.002"},{"v":80.48181170971604,"d":"80 "},"No",{"v":0.05,"d":"5.00%"},{"v":8.048181170971605e-05,"d":"0.008%"}]
[{"$nulls":5},"Other",null,"Butadiene copolymer","Trade secret",{"v":0.0006882460199999999,"d":"0.001"},{"v":24.144543512914815,"d":"24 "},"No",{"v":0.015,"d":"1.50%"},{"v":2.4144543512914814e-05,"d":"0.002%"}]
[{"$nulls":5},"Other",null,"Acrylate ","Trade secret",{"v":0.0027529840799999997,"d":"0.003"},{"v":96.57817405165926,"d":"97 "},"No",{"v":0.06,"d":"6.00%"},{"v":9.657817405165926e-05,"d":"0.010%"}]
[{"$nulls":5},"Other",null,"Epoxy resin","Trade secret",{"v":0.0011470767,"d":"0.001"},{"v":40.24090585485802,"d":"40 "},"No",{"v":0.025,"d":"2.50%"},{"v":4.0240905854858024e-05,"d":"0.004%"}]
[{"$nulls":5},"Other",null,"Peroxide","Trade secret",{"v":0.00022941534,"d":"0.000"},{"v":8.048181170971606,"d":"8 "},"No",{"v":0.005,"d":"0.50%"},{"v":8.048181170971606e-06,"d":"0.001%"}]
[{"$nulls":5},"Other",null,"Additive","Trade secret",{"v":0.0006882460199999999,"d":"0.001"},{"v":24.144543512914815,"d":"24 "},"No",{"v":0.015,"d":"1.50%"},{"v":2.4144543512914814e-05,"d":"0.002%"}]
[null,"Copper Wire","NIPPON","EX-SERIES",{"v":0.0279351129455591,"d":"0.028"},"Other",null,"Copper(Cu)","7440-50-8",{"v":0.027932319434264545,"d":"0.028"},{"v":979.9012016040956,"d":"980 "},"No",{"v":0.9999,"d":"99.99%"},{"v":0.0009799012016040956,"d":"0.098%"}]
[{"$nulls":5},"Other",null,"Palladium(Pd)","7440-05-3",{"v":2.7935112945559104e-06,"d":"0.000"},{"v":0.09799992015242483,"d":"0 "},"No",{"v":0.0001,"d":"0.01%"},{"v":9.799992015242483e-08,"d":"0.000%"}]
[null,"Molding compound","SD","CEL-9240HF",{"v":12.1956853324896,"d":"12.196"},"Other",null,"Epoxy resin1","Trade secret",{"v":0.30489213331224,"d":"0.305"},{"v":10696.002832683005,"d":"10,696 "},"No",{"v":0.025,"d":"2.50%"},{"v":0.010696002832683005,"d":"1.070%"}]
[{"$nulls":5},"Other",null,"Epoxy resin2","Trade secret",{"v":0.182935279987344,"d":"0.183"},{"v":6417.601699609802,"d":"6,418 "},"No",{"v":0.015,"d":"1.50%"},{"v":0.006417601699609803,"d":"0.642%"}]
[{"$nulls":5},"Other",null,"Hardener","Trade secret",{"v":0.426848986637136,"d":"0.427"},{"v":14974.403965756206,"d":"14,974 "},"No",{"v":0.035,"d":"3.50%"},{"v":0.014974403965756207,"d":"1.497%"}]
[{"$nulls":5},"Other",null,"Catalyst","Trade secret",{"v":0.0060978426662448,"d":"0.006"},{"v":213.92005665366008,"d":"214 "},"No",{"v":0.0005,"d":"0.05%"},{"v":0.00021392005665366007,"d":"0.021%"}]
[{"$nulls":5},"Other",null,"Carbon black","1333-86-4",{"v":0.0243913706649792,"d":"0.024"},{"v":855.6802266146403,"d":"856 "},"No",{"v":0.002,"d":"0.20%"},{"v":0.0008556802266146403,"d":"0.086%"}]
[{"$nulls":5},"Other",null,"Amorphous silica1","60676-86-0",{"v":9.75654826599168,"d":"9.757"},{"v":342272.09064585617,"d":"342,272 "},"No",{"v":0.8,"d":"80.00%"},{"v":0.3422720906458562,"d":"34.227%"}]
[{"$nulls":5},"Other",null,"Amorphous silica2","7631-86-7",{"v":1.493971453229976,"d":"1.494"},{"v":52410.41388014672,"d":"52,410 "},"No",{"v":0.1225,"d":"12.25%"},{"v":0.05241041388014672,"d":"5.241%"}]
[null,"Lead finish \n(Matte Sn) on leadframe","Tinking","Sn 99.99%",{"v":0.2548932672,"d":"0.255"},"Other",null,"Pure tin(Sn)","7440-31-5",{"v":0.2548932672,"d":"0.255"},{"v":8941.97917927578,"d":"8,942 "},"No",{"v":1,"d":"100%"},{"v":0.008941979179275781,"d":"0.894%"}]
[null,"DIE","SMIC","silicon",0.226716336,"Other",null,"Silicon ","7440-21-3",{"v":0.226243859155776,"d":"0.226"},{"v":7936.921599512344,"d":"7,937 "},"No",{"v":0.997916,"d":"99.79%"},{"v":0.007936921599512344,"d":"0.794%"}]
[{"$nulls":5},"Other",null,"Others","Trade Secret",{"v":0.00047247684422399425,"d":"0.000"},{"v":16.575087094889273,"d":"17 "},"No",{"v":0.0020839999999999748,"d":"0.21%"},{"v":1.6575087094889274e-05,"d":"0.002%"}]
[]
[]
[]
[]
[null," Giantec fill in"]
[null,"Supplier or Manufacturing Site fill in"]

{"sheet":"Abbreviations","index":2,"n_rows":51,"n_cols":5,"rows_kept":51,"flags":["formulas_cached_only"]}
["Termination Material Composition:",null,null,"Leadframe (Underplate) Material:"]
["Value","Description",null,"Value","Description"]
["Pure matte tin","100% Sn (matte) - no Ni barrier or annealing (Heat treatment)",null,"Alloy 42","Iron-based leadframe material"]
["Pure matte tin – annealed","100% Sn (matte), annealed is a heat treatment (e.g. 150°C for 1 hour)",null,"Copper","Cu, C194, C151, C7025"]
["Pure matte tin – reflowed","100% Sn (matte), reflowed indicates plating was completely melted after application",null,"Beryllium Copper","Be/Cu"]
["Pure matte tin - Ni barrier","100% Sn (matte), a nickel layer is added between the plating and base metal",null,"Brass","Cu/Zn alloy"]
["Pure matte tin - Ag barrier","100% Sn (matte), a silver layer is added between the plating and base metal",null,"Phosphor Bronze","P-Bronze"]
["Pure matte tin – fused","100% Sn (matte), fusing is a reflow operation in a hot oil bath",null,"Nickel","Ni (Used as barrier layer)"]
["Pure matte tin - reflowed over Nickel barrier","100% Sn (matte), reflowed over a nickel layer",null,"Kovar","Iron/Nickel based material"]
["Pure bright tin","100% Sn (bright) - no Ni barrier or annealing (Heat treatment)",null,"Other - please give details in Comments","To specify on Comment column"]
["Pure bright tin – annealed","100% Sn (bright), annealed is a heat treatment (e.g. 150°C for 1 hour)"]
["Pure bright tin – reflowed","100% Sn (bright), reflowed indicates plating was completely melted after application",null,"RoHS Exemptions:"]
["Pure bright tin - Ni barrier","100% Sn (bright), a nickel layer is added between the plating and base metal",null,"Value","Description"]
["Pure bright tin - Ag barrier","100% Sn (bright), a silver layer is added between the plating and base metal",null,1,"Mercury in compact fluorescent lamps not exceeding 5 mg per lamp"]
["Pure bright tin – fused","100% Sn (bright), fusing is a reflow operation in a hot oil bath",null,"2a","Mercury in straight fluorescent lamps for general purposes not exceeding halophosphate 10mg"]
["Pure bright tin - reflowed over Nickel barrier","100% Sn (bright), reflowed over a nickel layer",null,"2b","Mercury in straight fluorescent lamps for general purposes not exceeding triphosphate with normal lifetime 5 mg"]
["Semi-matte tin","100% Sn, material properties fall in between matte and bright conditions",null,"2c","Mercury in straight fluorescent lamps for general purposes not exceeding triphosphate with long lifetime 8 mg"]
["Nickel/Palladium/Gold","Ni/Pd/Au",null,3,"Mercury in straight fluorescent lamps for special purposes"]
["Nickel/Palladium","Ni/Pd",null,4,"Mercury in other lamps not specifically mentioned in this list"]
["Tin/Silver/Copper","Sn/Ag/Cu",null,5,"Lead in glass of cathode ray tubes, electronic components and fluorescent tubes"]
["Hot Dipped Tin/Silver/Copper","Sn/Ag/Cu applied in a molten tin bath process",null,"6a","Lead as an alloying element in steel containing up to 0.35% lead by weight"]
["Tin/Silver","Sn/Ag",null,"6b","Lead as an alloying element in aluminium containing up to 0.40% lead by weight"]
["Hot Dipped Tin/Silver","Sn/Ag applied in a molten tin bath process",null,"6c","Lead as a copper alloy containing up to 4.0% lead by weight"]
["Tin/Copper","Sn/Cu",null,"7a","Lead in high melting temperature type solders (i.e. lead-based solder alloys containing 85 % by weight or more lead)"]
["Hot Dipped Tin/Copper","Sn/Cu applied in a molten tin bath process",null,"7c","Lead in electronic ceramic parts (e.g. piezoelectronic devices)"]
["Tin/Copper – annealed","Sn/Cu, annealed is a heat treatment (e.g. 150°C for 1 hour)",null,8,"Cadmium and its compounds in electrical contacts and cadmium plating except for applications banned under Directive 91/338/EEC amending Directive 76/769/EEC relating to restrictions on the marketing and use of certain dangerous substances and preparations"]
["Tin/Lead","Sn/Pb",null,9,"Hexavalent chromium as an anti-corrosion of the carbon steel cooling system in absorption refrigerators"]
["Tin/Lead/Silver","Sn/Pb/Ag",null,"9a","DecaBDE in polymeric applications"]
["Nickel/Gold","Ni/Au",null,"9b","Lead in lead-bronze bearing shells and bushes"]
["Tin/Bismuth","Sn/Bi",null,11,"Lead used in compliant pin connector systems"]
["Silver/Palladium","Ag/Pd",null,12,"Lead as a coating material for a thermal conduction module c-ring"]
["Silver/Palladium - Ni barrier","Ag/Pd, a nickel layer is added between the plating and base metal",null,"13a","Lead in optical and filter glass"]
["Silver - Ni barrier","100% Ag, a nickel layer is added between the plating and base metal",null,"13b","Cadmium in optical and filter glass"]
["Gold","100% Au",null,14,"Lead in solders consisting of more than two elements for the connection between the pins and the package of microprocessors with a lead content of more than 80% and less than 85% by weight"]
["Gold over Nickel","Au plated over a Ni-barrier layer",null,15,"Lead in solders to complete a viable electrical connection between semiconductor die and carrier within integrated circuit Flip Chip packages"]
["Nickel","100% Ni",null,"N/A","Not Applicable"]
["Immersion Silver","Imm. Ag"]
["Immersion Tin","Imm. Sn"]
["Electroplated Silver","100% Ag",null,"Moisture Sensitivity:"]
["OSP","Organic polymer over copper",null,"Value","Description"]
["Hot Dipped Tin","100% Sn applied in a molten tin bath process",null,1]
["Zinc","100% Zn or Zn-alloy",null,2]
["Tin/Zinc","Sn plated over Zn",null,"2a"]
["Aluminum","100% Al",null,3]
["Indium alloy","In bearing alloy",null,4]
["Tin/Copper HASL","Sn/Cu Hot Air Solder Leveled",null,5]
["ENIG","Electroless Nickel Immersion Gold",null,"5a"]
["ENEPIG","Electroless Nickel/Electroless Palladium/Immersion Gold",null,6]
["Other - Please give details in Comments","To  specify on Comment column",null,"ANR","Affected (by moisture exposure), no JEDEC rating"]
[{"$nulls":3},"NMS","Not Moisture Sensitive"]
[{"$nulls":3},"IPC/JEDEC J-STD-020C; go to www.jedec.org"]